
Packet Tracer – Investigating DUAL FSM (Instructor Version)

**Instructor Note**: Red font color or Gray highlights indicate text that appears in the instructor copy only.

1. Topology



1. Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| R1 | G0/0 | 172.16.1.254 | 255.255.255.0 | N/A |
| S0/0/0 | 172.16.3.1 | 255.255.255.252 | N/A |
| S0/0/1 | 192.168.10.5 | 255.255.255.252 | N/A |
| R2 | G0/0 | 172.16.2.254 | 255.255.255.0 | N/A |
| S0/0/0 | 172.16.3.2 | 255.255.255.252 | N/A |
| S0/0/1 | 192.168.10.9 | 255.255.255.252 | N/A |
| R3 | G0/0 | 192.168.1.254 | 255.255.255.0 | N/A |
| S0/0/0 | 192.168.10.6 | 255.255.255.252 | N/A |
| S0/0/1 | 192.168.10.10 | 255.255.255.252 | N/A |
| PC1 | NIC | 172.16.1.1 | 255.255.255.0 | 172.16.1.254 |
| PC2 | NIC | 192.168.1.1 | 255.255.255.0 | 192.168.1.254 |
| PC3 | NIC | 192.168.2.1 | 255.255.255.0 | 192.168.2.254 |

1. Objectives

Part 1: Verify the EIGRP Configuration

Part 2: Observe the EIGRP DUAL FSM

1. Background

In this activity, you will modify the EIGRP metric formula to cause a change in the topology. This will allow you to see how EIGRP reacts when a neighbor goes down due to unforeseen circumstances. You will then use the **debug** command to view topology changes and how the DUAL Finite State Machine determines successor and feasible successor paths to re-converge the network.

1. Verify EIGRP Configuration
   1. Examine the routing tables of each router and verify that there is a path to every network in the topology.

What command displays the routing table? **show ip route**

Are any of the routers load balancing between any network? Yes, R1 to the 192.168.10.8 network, R2 to the 192.168.10.4 network, and R3 to the 172.16.3.0 network.

* 1. Verify that each router has entries in its neighbor table.

What command displays the neighbor table? **show ip eigrp neighbors**

How many neighbors does each router have? All routers have two neighbors.

* 1. Analyze the topology table of each router.
     1. What command displays the topology table? **show ip eigrp topology**

Based on the output in the topology table, how many successor paths does each router have? 7

Why are there more successor paths than networks? There are 6 networks in the topology but each router has two successor paths to one network (R1 has 2 successor paths to 192.168.10.8).

* + 1. Copy the output for **R1**'s topology table to a text editor so that you can refer to it later.

1. Observe the EIGRP DUAL FSM
   1. On R1, turn on the debugging feature that will display DUAL FSM notifications.

What command enables debugging for the EIGRP DUAL FSM? **debug eigrp fsm**

* 1. Force a DUAL FSM update to generate debug output.
     1. Place the R1 and R3 windows side by side so that you can observe the debug output. Then on R3, disable the serial 0/0/0 interface.

R3(config)# **interface s0/0/0**

R3(config-if)# **shutdown**

* + 1. Do not disable debugging yet. What debug output indicated changes to the routing table?

<output omitted>

DUAL: Dest 192.168.10.4/30 (No peers) not entering active state.

DUAL: Removing dest 192.168.10.4/30, nexthop 0.0.0.0

DUAL: No routes. Flushing dest 192.168.10.4/30

* 1. Display the routing table of R1.

Verify that 192.168.10.4/30 network is no longer in **R1**’s routing table.

Describe any other changes to the **R1** routing table? The 192.168.10.8 only has one route instead of two.

* 1. Determine the difference in the topology table.

Examine the topology table of **R1** and compare it to the previous output from Part 1.

Are there any other changes to the **R1**’s topology table? Yes, The 192.168.10.4/30 is no longer in the topology table and there is only one successor to the 192.168.10.8/30.

* 1. Document changes in each router’s neighbor table.

Examine the neighbor table of each router and compare it to the previous one from Part 1.

Are there any changes to the neighbor table? Yes, R1 192.168.10.6 no longer has R3 192.168.10.5 as a neighbor.

* 1. Restore connectivity between R1 and R2.
     1. With the R1 and R3 windows side by side, on R3 activate the serial 0/0/0 interface and observe the debug output on R1.
     2. Disable debugging by entering the **no** form of the debug command or simply enter **undebug** all. What debug output indicated changes to the routing table?

DUAL: Find FS for dest: 192.168.1.0/24. FD is 2682112, RD is 2170112

DUAL: RT installed 192.168.1.0/24 via 192.168.10.6

How did the DUAL FSM handle the change in topology when the route to **R1** came back up? The route between R1 and R3 on network 192.167.10.4/30 came back up and adjacencies were formed.

1. Suggested Scoring Rubric

|  |  |  |  |
| --- | --- | --- | --- |
| Activity Section | Question Location | Possible Points | Earned Points |
| Part 1: Verify EIGRP Configuration | Step 1 | 12 |  |
| Step 2 | 12 |  |
| Step 3 | 12 |  |
| **Part 1 Total** | | **36** |  |
| Part 2: Observe the EIGRP DUAL FSM | Step 1 | 10 |  |
| Step 2 | 12 |  |
| Step 3 | 10 |  |
| Step 4 | 10 |  |
| Step 5 | 10 |  |
| Step 6 | 12 |  |
| **Part 2 Total** | | **64** |  |
| **Total Score** | | **100** |  |